B L I N K Y - 1   K i n e t i c   P o e t r y   o n   t h e   P D P - 1
-----------------------------------------------------------------------
TW0>    *fun *Special function   SENSE SWITCH (SSn) ON ->
TW1>     cAC  Complement AC      SS1 = RIM-load halts CPU after loading
TW2>     cIO  Complement IO      SS2 = Restart BLINKY-1 if changed
TW3>     pPF  PF pattern (0,1)   SS3 = Don't use extended memory
TW4>     pAC  AC pattern (0,1)   SS4 = Print HELP text to the console
TW5>     pIO  IO pattern (0,1)   SS5 = Set tick (TK) speed from TW6-17
TW6-8>   sPF  PF speed (x sCK)   SS6 = CRT display (TYPE 30) enabled
TW9-11>  sAC  AC speed (x sCK)   --------------------------------------
TW12-14> sIO  IO speed (x sCK)   TW=135xxx -> Easter eggs     (Try SS6)
TW15-17> sCK  Basic clock speed  TW=77xxxx -> Flash all lamps (See SS5)
-----------------------------------------------------------------------
TEST WORD (TW) settings to try (begin with SS6=OFF) ->
135037  BLINKY-1 will 'read' you it's own binary code (SS6=ON after)
330000 'big fast loop'        010000 'reversal'
070000 'fast rotation'        000320 'bouncing'
TYPE 30 CRT display 'Easter egg' -> Turn SS6=ON and set the TW to ->
135007 'rocket'        136007 'missile'        122007 'sky rockets'
131007 'rockets'       137007 'dots'           123007 'streak'
133007 'satellites'    127007 'sky streaks'    121007 'streaks'
132007 'missiles'      126007 'fireworks'      TW0=ON to end Easter egg
